Revision: 0.0.2

Contents

===========

1 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

1.1 Explanation of symbols . . . . . . . . . . .2

1.2 Safety precautions . . . . . . . . . . . . . . .2

# 1 Introduction

* 1. **Explanation of symbols**

Warning symbols Key words indicate the seriousness of the hazard in terms of the consequences of not following the safety instructions. • NOTICE indicates possible damage to property or equipment, but where there is no risk of personal injury. • CAUTION indicates possible personal injury. • WARNING indicates possible severe personal injury

* 1. **Safety precautions**

**Oil fumes or leaks from the boiler:**

• Extinguish any naked flames.

• Open windows and doors.

• Switch off the boiler electricity supply.

• Isolate the fuel supply to the boiler.

• Contact installer/service engineer.

**This boiler must only be operated by a responsible adult who has been instructed in, understands and is aware of the boiler’s operating conditions and effects.**

Health and safety The appliance contains no asbestos and no substances have been used in the construction process that contravene the COSHH Regulations (Control of Substances Hazardous to Health Regulations 1988). Where applicable, the CE mark indicates compliance with relative EU Directives.